*** Rotterdam Atmospheric Measurement Network RAMN - Davis006 weather station data at EUR Campus ***

1. General information

1.1 Title: Rotterdam Atmospheric Measurement Network RAMN - Davis006 weather station data at EUR campus 
1.2 Description: Each file covers a full month of observations. The temporal resolution is 1 minute. Data are provided "as is", without any modifications
1.3 File naming convention: Sensor_Location_YYYYMM.nc
1.4 Contact person: Marc Schleiss, m.a.schleiss@tudelft.nl

2. Methodological information

2.1 Data acquisition: The data were collected by a Davis vantage Pro2 weather station operated by the TU Delft within the context of the Rotterdam Atmospheric Measurement Network RAMN Initiative, in collaboration with the Ruisdael Observatory. 
2.2 logging software: Data acquisition is done through a RaspberryPi computer running the "WeeWX" software (https://weewx.com/). The temporal resolution is 1 minute.
2.3 Data processing: By default, the logging software generates a daily NetCDF file. A small R script then reads and aggregates these daily data into monthly files for publication. Data are provided "as-is", and come without warranty. Please report any issues you notice to the authors.

3. Data specific information

3.1 Metadata: Each NetCDF file contains the short names, full names, units and missing_value attributes of the variables.
3.2 Main contributors: Marc Schleiss, Mahaut Sourzac, Marjolein van Esch, Jelle Burger, Rob Mackenzie, Andre Castro

4. Sharing and Access information

Data license: CC BY 4.0 https://creativecommons.org/licenses/by-sa/4.0/" 



