*** EDoM measurement campaign: data from bottom mounts ***
Authors: Bas van Maren, Julia Vroom, Daan van Keulen, Christian Maushake
Corresponding author: bas.vanmaren@deltares.nl

*** GENERAL INFORMATION ***
Subset of larger dataset collected during the Ems Dollard Measurements (EDoM) Campaign in 2018 and 2019. This subset contains data collected by so-called bottom-mounts (frames installed on the ground with one upward looking ADCP and an OBS sensor)
It is composed of 10 files, each file containing the measurements collected on one location (5 in total) during one field campaign (2 in total). 

Filenemame convention: BM_<loc>_<year>.nc, where 
- BM is bottom mount, 
- <loc> is the location (GEI, EFW, GAT, KNO, DOL), 
- <year> is 2018 or 2019. 
See accompanying report(report-EDoM_v2.0.pdf) for location of stations.


*** METHODOLOGICAL INFORMATION ***
See accompanying report(report-EDoM_v2.0.pdf) for details.

*** DATA SPECIFIC INFORMATION ***

Each file contains
1. x
  description = "x-coordinate [m] (UTM 32)";  
  Units = "m";
2. y
  description = "y-coordinate [m] (UTM 32)";  
  Units = "m";
3. h_con
  description = "height of ADCPs above the bed, i.e. TRBM height";
  Units = "m";
4. time;
  description = "(Matlab) Serial date number  represents the whole and fractional number of days from 01-01-0000";  
  Units = "days since 01-01-0000";
5. Sal
  description = "10 minute averaged salinity";
  Units = "ppt";
6. SSC
  description = "10 minute averaged suspended sediment concentration";
  Units = "mg/l";
7. Temp
  description = "10 minute averaged temperature";  
  Units = "degrees C";
8. Turb;
  description = "10 minute averaged turbidity";
  Units = "NTU";
9. vel_East;
  description = "10 minute bin averaged velocity in the Eastward direction";
  Units = "m/s";
10. vel_North;
  description = "10 minute bin averaged velocity in the northward direction";
  Units = "m/s";  
11. backscatter_10av
  description = "10 minute averaged absolute backscatter";
  Units = "dB";
12. deviceDepth_10av
  description = "10min averaged water depth at TRBM";
  Units = "m";