*** EDoM measurement campaign: floc data measured at SB_EMD
Authors: Andy Manning and Bas van Maren
contact: Andy Manning <andymanning@yahoo.com>

*** GENERAL INFORMATION ***
Floc settling velocity observations using an onboard floc camera. Water samples collected with a Niskin bottle, subsampled onboard and inserted into settling ccolumn with camera. 
Postprocessing of data in a later stage to extract floc properties per water sample. 

*** DATA SPECIFIC INFORMATION ***

Data is stored in text files containing the follwoing information:
- Size (microns)	
- Effective Density (kg/m^3)	
- Ws (mm/s)	
- nf	
- H_W_ratio	
- Porosity

One file per water sample, following the following convention for the filename [A/S <number> b/s ].txt: 

A        = August 2018
B        = January 2019
<number> = chronological order: see ambient conditions and time below 
s        = surface sample (~0.5m below surface)
b        = bed sample (~0.5m above bed)


August
Sample	Time (UTC)	SSC (mg/l)
A01s	09:07	130
A02b	09:29	390
A03s	09:44	280
A04b	10:13	500
A05s	10:54	410
A06b	11:08	540
A07s	11:50	340
A09s	13:06	180
A10b	13:40	170
A11s	14:19	110
A12b	15:17	110
A13s	16:02	330
A14b	16:34	360
A15s	17:06	310
A17s	18:31	300
A18b	19:12	320
A19s	19:42	260
A20b	20:07	390
A23b	21:47	90


January 
Sample	Time (UTC)	SSC (mg/l)
J01s	08:52	4100
J03s	09:42	2200
J05s	11:02	1017
J06b	11:46	3100
J07s	12:02	520
J08b	12:38	2600
J11s	14:04	277
J12b	14:27	545
J13s	15:00	158
J14b	15:32	185
J15s	15:56	154
J16b	16:45	440
J17s	17:03	220
J18b	17:37	1697
J19s	18:05	877
J21s	19:05	1507
J22b	19:38	1987
J23s	20:04	2233
J24b	20:39	2600
